{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":1,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":77,"n_cols":2,"rows_kept":77,"cut":false,"hidden":false,"merged":[]}
[]
[null,"570ST"]
["ENGINE"]
["Model code ","TCA8040.45"]
["Type ","TCA"]
["Bore / Stroke ","104 x 115 mm"]
["Displacement / Compression ratio ","3.9 l / 18.3:1"]
["Horsepower ","97 hp"]
["Maximum torque ","420 Nm"]
["Engine speeds ","2200 rated speed, full load, 950 low idle speed (at no load)"]
["POWER TRAIN"]
["Transmission ","CARRARO 2WD TLB1 or 4WD TLB1"]
["Model ","CARRARO 4WD TLB1 (for 570T/ST 4WD)"]
["Type ","Power Shuttle with 4 forward and 4 reverse travel gears"]
["Gear ","Forward - Reverse (speed kmph)"]
["1st - 2nd - 3rd - 4th ","7.4 - 12 - Not recom. - Not recom."]
["FRONT AXLE"]
["2 Wheel Drive (Standard) ","Model CNH PS1300"]
["Type - Oscillation ","Steering - +/- 8 °"]
["4 Wheel Drive (Optional) ","Model CARRARO 26.17"]
["REAR AXLE"]
["Model for 570T 2WD and 4WD ","CARRARO 28.32M"]
["Type ","Rigid"]
["BRAKES"]
["Service Brakes ","Type: wet multi-discs / Nr. of discs: 6"]
["Parking Brakes ","Type: Manual, with lever"]
["TYRE SIZE RECOMMENDED"]
["2WD ","16.9 x 28 - 12PR or 14 x 25 - 20PR rear"]
["4WD ","16.9 x 28 - 12PR rear"]
["TRANSMISSION"]
["Powershuttle: Forward speeds ","-"]
["Reverse speeds ","-"]
["Powershift: Forward speeds ","-"]
["Powershift: Reverse speeds ","-"]
["HYDRAULIC SYSTEM"]
["Type ","Closed center with double gear pump"]
["Flow rate ","145 lpm @ 2200 rpm"]
["Pressure ","210 bar"]
["STEERING"]
["Type ","Power Steering"]
["System pressure / Displacement ","140 bar / 125 cc"]
["Turning radius (outside of the bucket) ","5550 mm without brake"]
["Tread width ","1697 mm rear"]
["BATTERY"]
["Battery ","-"]
["CABIN"]
["Certification ","ROPS/FOPS"]
["Air conditioning ","Optional"]
["OPERATING WEIGHT"]
["4 WD, standard dipper/Ext. ","-"]
["4 WD, extendible dipper/Ext ","-"]
["SERVICE CAPACITIES"]
["Engine oil ","11 ltr"]
["Transmission oil ","16 ltr"]
["Rear axle oil ","18 ltr"]
["Hydraulic oil ","130 ltr"]
["Fuel tank ","142 ltr"]
["Coolant ","20 ltr"]
["TURNING RADIUS"]
["Front tires 12.5/80-18, wheel not braked, 4WD engaged ","-"]
["AXLES, TIRES & BRAKE"]
["Brake ","-"]
["Front tires ","-"]
["Rear tires ","-"]
["Front axle: oscillation of +/- 11° ","-"]
["EMISSIONS (g/kWh)"]
["CO² emission ","-"]
["NOx emission ","-"]
["HC emission ","-"]
["CO emission ","-"]
["PM emission ","-"]
["NOx + HCNM emission ","-"]
["NOISE"]
["Internal dB(A) ","-"]
["External dB(A) ","-"]
["VIBRATION LEVELS"]
["Vibration levels ","-"]